IOTC Platform: st_RDT_Status Struct Reference

| IOTC Platform Ver: 2.1.0.25 |

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros
Data Fields
st_RDT_Status Struct Reference

`#include <RDTAPIs.h>`

## Data Fields

unsigned short | Timeout
| The remaining time, in unit of second, to keep the RDT channel alive.
unsigned short | TimeoutThreshold
| RDT channel will be terminated if timeout exceeds this threshold, in unit of seconds.
unsigned int | BufSizeInSendQueue
| The size, in unit of byte, of buffer remaining in the sending queue in the local site.
unsigned int | BufSizeInRecvQueue
| The size, in unit of byte, of buffer remaining in the receiving queue in the local site.

## Detailed Description

RDT channel status, containing the current status of a RDT channel created between a RDT server and a RDT client. Users can use RDT_Status_Check() to get RDT status.

## Field Documentation

unsigned int BufSizeInRecvQueue

The size, in unit of byte, of buffer remaining in the receiving queue in the local site.

unsigned int BufSizeInSendQueue

The size, in unit of byte, of buffer remaining in the sending queue in the local site.

unsigned short Timeout

The remaining time, in unit of second, to keep the RDT channel alive.

unsigned short TimeoutThreshold

RDT channel will be terminated if timeout exceeds this threshold, in unit of seconds.

The documentation for this struct was generated from the following file:

- RDTAPIs.h