IOTC Platform: st_LanSearchInfo2 Struct Reference

| IOTC Platform Ver: 2.1.0.25 |

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros
Data Fields
st_LanSearchInfo2 Struct Reference

`#include <IOTCAPIs.h>`

## Data Fields

char | UID [21]
| The UID of discovered device.
char | IP [16]
| The IP address of discovered device.
unsigned short | port
| The port number of discovered device used for IOTC session connection.
char | DeviceName [132]
| The Name of discovered device.
char | Reserved
| Reserved, no use.

## Detailed Description

Device search info, containing all the information and device name when client searches devices in LAN.

## Field Documentation

char DeviceName[132]

The Name of discovered device.

char IP[16]

The IP address of discovered device.

unsigned short port

The port number of discovered device used for IOTC session connection.

char Reserved

Reserved, no use.

char UID[21]

The UID of discovered device.

The documentation for this struct was generated from the following file:

- IOTCAPIs.h